RFP 23-05		 January 26, 2023
Bid Form

ADDENDUM NO. 2

BID NO.  23-05
SEWER REHABILITATION 
(GILES LANE & ROUTE 40 AREAS)

To all holders of the specifications, the following corrections are hereby made.  All other items shall remain unchanged. This addendum shall become part of the Contract Documents for the above referenced project. 

Acknowledgement of Addendum

Name: ___________________________________________________

Company: ________________________________________________

Date: ____________________________________________________

Signature: ________________________________________________


Q1: Do you have any profile sheets or anything showing depth of the sewer lines requiring rehabilitation?  Can you also confirm that all manholes requiring rehab are standard 48” diameter?
A1:  The only info available is manhole depths as shown in the table below.  The manholes are at least the standard size of 48” if not larger.  
	MANHOLE ID 
	INVERT
	ELEVATION

	SMH-1244
	169.4
	178.337

	SMH-1120
	168.4
	175.906

	SMH-1119
	166.5
	182.706

	SMH-0001
	 - 
	 - 

	SMH-1050
	166.5
	175.447

	SMH-1245
	164.8
	172.061

	SMH-1246
	164.3
	170.553

	SMH-1665
	 - 
	 - 

	SMH-0459
	161.1
	168.417

	SMH-0434
	159.5
	167.041

	SMH-1090
	157.1
	168.609

	SMH-0435
	154.9
	164.045

	SMH-0365
	151.3
	158.807

	SMH-0436
	147.4
	156.252

	SMH-1424
	146.6
	150.998
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