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Bid Form

ADDENDUM NO. 3

BID NO.  23-01

STREET RESURFACING, AND REMOVAL & REPLACEMENT OF CONCRETE CURB, GUTTER, SIDEWALK AT VARIOUS LOCATIONS IN THE CITY OF ABERDEEN, MARYLAND

To all holders of the specifications, the following corrections are hereby made.  All other items shall remain unchanged. This addendum shall become part of the Contract Documents for the above referenced project. 

Acknowledgement of Addendum

Name: ___________________________________________________

Company: ________________________________________________

Date: ____________________________________________________

Signature: ________________________________________________

· Section 1: Answers to Questions Posed by Bidders

Q1: SPG-1, 1.1.1 Resurfacing calls for 1.5” of milling and paving.  It is again called out on SPG-2, 2.2.1 Paving Procedure.  However, item 504 calls for 2” Surface but the quantities of milling and paving, given, equate to 1.5”.  Please advise as to which depth we are to use.?

A1: Unit Price will be determined using a depth of 2”.  

· Section 2: Corrections to Specifications

SPG1-1, 1.1.1 shall read: “The work to be done under these specifications generally consists of, but not limited to, patching, raising existing utility covers, milling of existing paving to a depth of two (2) inches at existing cross street tie in and along the existing gutter pan, assuring the street surface is cleaned, application of tack coat, and the application of approximately 5,000 tons of bituminous concrete surface (Band SF) to a depth of two (2) inches or greater after compaction.”

SPG-2, 2.2.1 shall read: “The contractor is responsible for total roadway surface preparation for pavement operations.  The finished roadway shall have a uniform cross slope with a smooth, even surface.  This will be achieved by placing a two (2) inch average (unless otherwise noted) overlay of Bituminous Concrete Band SF and, if necessary, by placing a wedge and leveling course of the same prior to the overlay course.

· Section 3: Bid Form Revision – Rev 1

Bid Form Line Item 504 	Approx Qty Changed from 5,000 TON to 6,600 TON 
		CITY OF ABERDEEN

		CITY OF ABERDEEN

