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ADDENDUM NO. 5


BID NO.  23-05
SEWER REHABILITATION 
(GILES LANE & ROUTE 40 AREAS)


To all holders of the specifications, the following corrections are hereby made.  All other items shall remain unchanged. This addendum shall become part of the Contract Documents for the above referenced project. 


Acknowledgement of Addendum

Name: ___________________________________________________

Company: ________________________________________________

Date: ____________________________________________________

Signature: ________________________________________________




Q1: What size is the main where the manholes are to be rehabilitated?
A1: Please see the table below for the size, material, and rough elevations:

	MANHOLE
	INVERT 
	ELEVATION
	INLET
	OUTLET

	SMH-0858
	61.62
	69.79
	8" PVC
	8" DIP

	SMH-0855
	58.38
	64.43
	8" PVC
	8" PVC

	SMH-1256
	56.82
	61.46
	8" PVC
	10" DIP

	SMH-0851
	56.34
	60.41
	10" DIP
	10" PVC

	SMH-0849
	55.78
	61.15
	10" PVC
	10" PVC

	SMH-0848
	55.21
	62.96
	10" PVC
	12" PVC



		

