August 14, 2025

ADDENDUM NO. 5

BID NO. 26-03

SEWER REHABILITATION
ANNUAL CONTRACT

To all holders of the specifications, the following corrections are hereby made. All other items shall remain unchanged. This addendum shall become part of the Contract Documents for the above referenced project.

Acknowledgement of Addendum

Name:	________________________________________________

Company:	________________________________________________

Date:		________________________________________________

Signature:	________________________________________________


Q1: 	For the 6 inch mainline pipe lining can another form of pipe lining be used other than UV cured? 

A1:	No. UV cure shall be used for all pipe lining within the scope.  That being said, we do not anticipate any mainlines smaller than 8” at this time.

