RFP 23-05		 January 9, 2023
Bid Form

ADDENDUM NO. 1

BID NO.  23-05
SEWER REHABILITATION 
(GILES LANE & ROUTE 40 AREAS)

To all holders of the specifications, the following corrections are hereby made.  All other items shall remain unchanged. This addendum shall become part of the Contract Documents for the above referenced project. 

Acknowledgement of Addendum

Name: ___________________________________________________

Company: ________________________________________________

Date: ____________________________________________________

Signature: ________________________________________________




Q1: Will the City accept UV Cured GRP lining on this project?
A1:  Yes.  The use of a UV Cured Glass Reinforced Pipe (i.e., Reline America Alphaliner, or comparable) is approved for use in City of Aberdeen sewer utilities. 
In the Bid Package, SPG-4.3.2.1 states that the lining product manufacturer must be certified to ISO 9001 (or equal) standards.  SPG-4.3.1 requires that data sheets on products are required as well.
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