RFP 23-04		 December 7, 2022
Bid Form

ADDENDUM NO. 1

BID NO.  23-04
POST RD SEWER REPLACEMENT

To all holders of the specifications, the following corrections are hereby made.  All other items shall remain unchanged. This addendum shall become part of the Contract Documents for the above referenced project. 

Acknowledgement of Addendum

Name: ___________________________________________________

Company: ________________________________________________

Date: ____________________________________________________

Signature: ________________________________________________




Q1: Can the bid opening be rescheduled to a time after the first of the year?
A1:  Yes.  The bid opening has been rescheduled to January 4th, 2023.


Q2: Can the project be started soon after notice to proceed? 
A2:  Yes. The awarded bidder will coordinate a schedule and start date at the time of notice to proceed.  The project can start as soon as logistically possible.  (This includes winter months if need.)

Q3: What are the specifics of traffic control required for this project? 
A3:  Traffic control will require a temporary closure and detour of a section of Post Rd.  The road closure will be coordinated with SHA and HCPS agencies.  Post Rd. can be closed for the duration of the work period each day but must be reopened at the end of each workday.  (The site will have to be stabilized and secured as well.)  Workday start and end times will be agreed upon at the time of pre-construction.  The coordination and setup of the detour and closure will be completed by City staff.


Q4: Will a staging area be provided near the project site? 
A4:  Yes.  A staging area can be provided at our DPW Maintenance Shop which is about a half a mile away from the site, near our WWTP Plant.  Specifics will be agreed upon at the pre-construction meeting.


Q5: What, if any, are the considerations regarding the condition of existing SMH-0746? 
A5:  The condition of existing SMH-0746 is less than satisfactory, but replacement of this manhole is not within the scope of this project.  The Contractor will need to replace the existing connection into SMH-0746 as required by existing conditions.  That being said, the Contractor is required to preserve the condition of the existing manhole for the duration of the project.

Q6: Will the proposed path of the new sewer line be too close to the water main and what slope should be used?
A6:  The path of the new sewer line shall be adjusted as needed to stay at the appropriate distance from the water main.  This can be accomplished while keep the area of disturbance limited to one side of the road.  To clarify the slope of the new pipe shall conform to the Harford County Sewer Main Design Guidelines for 8” pipe.  (Chap 4 25-75)

Q7: What paving and backfill requirements are within the scope of the project?
A7:  The excavated area shall be backfilled with select fill and paved according to details provided.  The disturbed roadway area from the centerline of Post Rd to the curb shall be resurfaced at the earliest availability after completion of the project.

Q8: Are geotechnical services required?
A8:  Yes, geotechnical services will be part of the City inspection process.

Q9: Are the manholes required to be lined?
A9:  Yes, all manholes within the City wastewater system are now specified to be lined with Duraplate or equivalent product.

Q10: Will flow control or bypass be necessary for this project?
A10:  Flow control from the three services on the main to be replaced should be minimal and will be the responsibility of the contractor to manage.  When connecting to existing SMH 0746, a temporary plug can be installed upstream by the City if need be.

Q11: Will the site be staked out or white-lined for the Contractor?
A11:  Yes, at the pre-construction phase of the project.  A site visit will be arranged, and the necessary items and locations can be marked and identified.  This includes the location of the service lateral that will have cleanouts installed as part of the scope of this project.
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